Response: AT+CGDCONT?

+CGDCONT: 1,"IP","v-internet","0.0.0.0",0,0,0,0

OK

APN duoc cau hinh thanh cong!.

Response: AT

OK

Response: AT+CGREG?

+CGREG: 0,1

OK

Response: AT+NETCLOSE

OK

+NETCLOSE: 0

Response: AT+CGDCONT=1,"IP","v-internet","0.0.0.0",0,0

OK

Response: AT+CIPMODE=0

OK

Response: AT+CIPSENDMODE=0

OK

Response: AT+CIPCCFG=10,0,0,0,1,0,75000

OK

Response: AT+CIPTIMEOUT=75000,15000,15000

OK

Response: AT+NETOPEN

OK

+NETOPEN: 0

Response: AT+NETOPEN?

+NETOPEN: 1

OK

Response: AT+CIPCLOSE=0

+CIPCLOSE: 0,4

ERROR

Response: AT+CIPOPEN=0,"TCP","visualizationenvironment.atwebpages.com",80

OK

+CIPOPEN: 0,0

Response: AT+CIPSEND=0,27

>

Response: POST /insert.php HTTP/1.1

OK

+CIPSEND: 0,27,27

Response: ationenvironment.atwebpages.com

Manufacturer: SIMCOM INCORPORATED

Model: SIMCOM\_SIM7600CE-M1S

ReHost: visualizationenvironment.atwebpages.com

Response: v

Response: ation/x-www-form-urlencoded

Manufacturer: SIMCOM INCORPORATED

Model: SIMCOM\_SIM7600CE-M1S

RevisiHost: visualizationenvironment.atwebpages.com

Response: o

Response:

Response:

Response:

Response: AT+CIPCLOSE=0

OK

+CIPCLOSE: 0,0

Response: AT++NETCLOSE

ERROR

log\_mã hai  
Response: AT+CGDCONT?

ERROR

APN cau hinh sai...

Response: AT+CGDCONT=1,"IP","v-internet","0.0.0.0",0,0

OK

Response: AT+CGDCONT?

+CGDCONT: 1,"IP","v-internet","0.0.0.0",0,0,0,0

OK

APN duoc cau hinh thanh cong!.

Response: AT

OK

Response: AT+CGREG?

+CGREG: 0,1

OK

Response: AT+NETCLOSE

OK

+NETCLOSE: 0

Response: AT+CGDCONT=1,"IP","v-internet","0.0.0.0",0,0

OK

Response: AT+CIPMODE=0

OK

Response: AT+CIPSENDMODE=0

OK

Response: AT+CIPCCFG=10,0,0,0,1,0,75000

OK

Response: AT+CIPTIMEOUT=75000,15000,15000

OK

Response: AT+NETOPEN

OK

+NETOPEN: 0

Response: AT+NETOPEN?

+NETOPEN: 1

OK

Response: AT+CIPCLOSE=0

+CIPCLOSE: 0,4

ERROR

Response: AT+CIPOPEN=0,"TCP","visualizationenvironment.atwebpages.com",80

OK

+CIPOPEN: 0,0

Response: AT+CIPSEND=0,27

>

Response: POST /insert.php HTTP/1.1

OK

+CIPSEND: 0,27,27

Response: AT+CIPSEND=0,47

>

Response: Host: visualizationenvironment.atwebpages.com

OK

Response: AT+CIPSEND=0,19

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,49

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,16

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,2

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,2

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,2

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,21

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,2

+CIPERROR: 4

ERROR

Response: AT+CIPCLOSE=0

+CIPCLOSE: 0,4

ERROR

Response: AT++NETCLOSE

ERROR

log\_3  
Response: AT+CGDCONT?

ERROR

APN cau hinh sai...

Response: AT+CGDCONT=1,"IP","v-internet","0.0.0.0",0,0

OK

Response: AT+CGDCONT?

+CGDCONT: 1,"IP","v-internet","0.0.0.0",0,0,0,0

OK

APN duoc cau hinh thanh cong!.

Response: AT

OK

Response: AT+CGREG?

+CGREG: 0,1

OK

Response: AT+NETCLOSE

+NETCLOSE: 2

ERROR

Response: AT+CGDCONT=1,"IP","v-internet","0.0.0.0",0,0

OK

Response: AT+CIPMODE=0

OK

Response: AT+CIPSENDMODE=0

OK

Response: AT+CIPCCFG=10,0,0,0,1,0,75000

OK

Response: AT+CIPTIMEOUT=75000,15000,15000

OK

Response: AT+NETOPEN

OK

+NETOPEN: 0

Response: AT+NETOPEN?

+NETOPEN: 1

OK

Response: AT+IPADDR

+IPADDR: 11.114.221.83

OK

Response: AT+CIPCLOSE=0

+CIPCLOSE: 0,4

ERROR

Response: AT+CIPOPEN=0,"TCP","nizarmohisim.atwebpages.com",80

OK

+CIPOPEN: 0,0

Response: AT+CIPSEND=0,27

>

Response: POST /insert.php HTTP/1.1

OK

+CIPSEND: 0,27,27

Response: AT+CIPSEND=0,35

>

Response: Host: nizarmohisim.atwebpages.com

OK

+CIPSEND: 0,35,35

Response: AT+CIPSEND=0,19

>

Response: Connection: close

OK

+CIPSEND: 0,19,19

Response: AT+CIPSEND=0,49

>

Response: Content-Type: application/x-www-form-urlencoded

OK

+CIPSEND: 0,49,49

Response: AT+CIPSEND=0,16

>

Response: Content-Length:

OK

+CIPSEND: 0,16,16

Response: AT+CIPSEND=0,2

>

Response: 20

OK

+CIPSEND: 0,2,2

Response: AT+CIPSEND=0,2

>

RECV FROM:185.176.43.104:80

+RECEIVE,0,391

HTTP/1.1 408 Request Timeout

Date:AT+CIPSEND=0,2

Response:

OK

Response: AT+CIPSEND=0,2

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,20

+CIPERROR: 4

ERROR

Response: AT+CIPSEND=0,2

+CIPERROR: 4

ERROR

Response: AT+CIPCLOSE=0

+CIPCLOSE: 0,4

ERROR

Response: AT++NETCLOSE

ERROR

Response: AT

OK

Response: AT+CGREG?

+CGREG: 0,1

OK

Response: AT+NETCLOSE

OK

+NETCLOSE: 0

Response: AT+CGDCONT=1,"IP","v-internet","0.0.0.0",0,0

OK

Response: AT+CIPMODE=0

OK

Response: AT+CIPSENDMODE=0

OK

Response: AT+CIPCCFG=10,0,0,0,1,0,75000

OK

Response: AT+CIPTIMEOUT=75000,15000,15000

OK

Response: AT+NETOPEN

OK

+NETOPEN: 0